diskdef ibm-3740
  seclen 128
  tracks 77
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 6
  boottrk 2
  os 2.2
end

diskdef 4mb-hd
  seclen 128
  tracks 1024
  sectrk 32
  blocksize 2048
  maxdir 256
  skew 1
  boottrk 0
  os p2dos
end

diskdef sdcard
  seclen 512
  tracks 256
  sectrk 64
  blocksize 8192
  maxdir 256
  skew 0
  boottrk 1
  os 2.2
end

diskdef pcw
  seclen 512
  tracks 40
  sectrk 9
  blocksize 1024
  maxdir 64
  skew 1
  boottrk 1
  os 3
  libdsk:format pcw180
end

diskdef pc1.2m
  seclen 512
  tracks 80
  # this format uses 15 sectors per track, but 30 per cylinder
  sectrk 30
  blocksize 4096
  maxdir 256
  skew 1
  boottrk 0
  os 3
end

# CP/M 86 on 1.44MB floppies
diskdef cpm86-144feat
  seclen 512
  tracks 160
  sectrk 18
  blocksize 4096
  maxdir 256
  skew 1
  boottrk 2
  os 3
  libdsk:format ibm1440
end

# CP/M 86 on 720KB floppies
diskdef cpm86-720
  seclen 512
  tracks 160
  sectrk 9 
  blocksize 2048
  maxdir 256
  skew 1
  boottrk 2
  os 3
end

diskdef cf2dd
  seclen 512
  tracks 160
  sectrk 9
  blocksize 2048
  maxdir 256
  skew 1
  boottrk 1
  os 3
  libdsk:format pcw720
end

#amstrad: values are read from super block (special name hardcoded)

# Royal alphatronic
# setfdprm /dev/fd1 dd ssize=256 cyl=40 sect=16 head=2
diskdef alpha
  seclen 256
  tracks 40
  sectrk 32
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# Apple II CP/M skew o Apple II DOS 3.3 skew
diskdef apple-do
  seclen 256
  tracks 35
  sectrk 16
  blocksize 1024
  maxdir 64
  skewtab 0,6,12,3,9,15,14,5,11,2,8,7,13,4,10,1
  boottrk 3
  os 2.2
end

# Apple II CP/M skew o Apple II PRODOS skew
diskdef apple-po
  seclen 256
  tracks 35
  sectrk 16
  blocksize 1024
  maxdir 64
  skewtab 0,9,3,12,6,15,1,10,4,13,7,8,2,11,5,14
  boottrk 3
  os 2.2
end

# MYZ80 hard drive (only works with libdsk, because it has a 256-byte header)
diskdef myz80
  seclen 1024
  tracks 64
  sectrk 128
  blocksize 4096
  maxdir 1024
  skew 1
  boottrk 0
  os 3
  libdsk:format pcw720
end

# Despite being Amstrad formats, CPC System and CPC Data don't have an Amstrad 
# superblock. You'll need to use libdsk to access them because the Linux 
# and Windows kernel drivers won't touch them.
diskdef cpcsys
  seclen 512
  tracks 40
  sectrk 9
  blocksize 1024
  maxdir 64
  skew 1
  boottrk 2
  os 3
  libdsk:format cpcsys
end
diskdef cpcdata
  seclen 512
  tracks 40
  sectrk 9
  blocksize 1024
  maxdir 64
  skew 1
  boottrk 0
  os 3
  libdsk:format cpcdata
end

# after being read in with no sector skew.
diskdef nigdos
  seclen 512
  # NigDos double sided disk format, 42 tracks * 2 sides
  tracks 84
  sectrk 10
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 0
  # this format wastes half of the directory entry
  logicalextents 1
  os 3
end

diskdef epsqx10
  seclen 512
  tracks 40
  sectrk 20
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

diskdef ibm-8ss
  seclen 512
  tracks 40
  sectrk 8
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 1
  os 2.2
end

diskdef ibm-8ds
  seclen 512
  tracks 40
  sectrk 8
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 1
  os 2.2
end

diskdef electroglas
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 256
  skew 0
  boottrk 1
  os 3
end

# IBM CP/M-86
# setfdprm /dev/fd1 sect=8 dtr=1 hd ssize=512 tpi=48 head=1
diskdef ibmpc-514ss
   seclen 512
   tracks 40
   sectrk 8
   blocksize 1024
   maxdir 64
   skew 1
   boottrk 1
   os 2.2
   libdsk:format ibm160
end

# IBM CP/M-86
# setfdprm /dev/fd1 sect=8 dtr=1 hd ssize=512 tpi=48
diskdef ibmpc-514ds
   seclen 512
   tracks 80
   sectrk 8
   blocksize 2048
   maxdir 64
   skew 0
   boottrk 2
   os 2.2
   libdsk:format ibm320
end

diskdef p112
  seclen 512
  tracks 160
  sectrk 18
  blocksize 2048
  maxdir 256
  skew 1
  boottrk 2
  os 3
end

diskdef p112-old
  seclen 512
  tracks 160
  sectrk 18
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 1
  os 3
end

diskdef gide-cfa
  seclen 512
  tracks 1000
  sectrk 16
  blocksize 4096
  maxdir 1024
  skew 0
  boottrk 2
  os 3
end

diskdef gide-cfb
  seclen 512
  tracks 1000
  sectrk 16
  blocksize 4096
  maxdir 1024
  skew 0
  boottrk 0
# Start of second partition
  offset 1000trk
  os 3
end

# AT&T/Olivetti Word Processor
diskdef attwp
   seclen 256
   tracks 80
   sectrk 32
   blocksize 2048
   maxdir 128
   boottrk 1
   logicalextents 1
   skewtab 0,2,4,6,8,10,12,14,1,3,5,7,9,11,13,15,16,18,20,22,24,26,28,30,17,19,21,23,25,27,29,31
   os 2.2
end

# setfdprm /dev/fd0 zerobased SS DD ssize=512 cyl=40 sect=10 head=1
# Kaypro II
diskdef kpii
  seclen 512
  tracks 40
  sectrk 10
  blocksize 1024
  maxdir 64
  dirblks 4
  skew 0
  boottrk 1
  os 2.2
end

# setfdprm /dev/fd0 zerobased DS DD ssize=512 cyl=40 sect=10 head=2
# Kayro IV
diskdef kpiv
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 64
  dirblks 2
  skew 0
  boottrk 1
  os 2.2
end

# setfdprm /dev/fd0 dd sect=10
diskdef interak
  seclen 512
  tracks 80
  sectrk 20
  blocksize 4096
  maxdir 256
  skew 1
  boottrk 2
  os 2.2
end

# Timex FDD3000 3"
diskdef fdd3000
  seclen 256
  tracks 40
  sectrk 16
  blocksize 1024
  maxdir 128
  boottrk 4
  os 2.2
  skew 7
end

# Timex FDD3000 3"
diskdef fdd3000_2
  seclen 256
  tracks 40
  sectrk 16
  blocksize 1024
  maxdir 128
  boottrk 2
  os 2.2
  skew 5
end

# Robotron 1715
diskdef 1715
  seclen 1024
  tracks 40
  sectrk 5
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 3
  os 2.2
end

# Robotron 1715 with SCP3
diskdef 17153
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 4
  os 3
end

#DDR
diskdef scp624
  seclen 256
  tracks 160
  sectrk 16
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

diskdef scp640
  seclen 256
  tracks 160
  sectrk 16
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 0
  os 2.2
end

diskdef scp780
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

diskdef scp800
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 0
  os 2.2
end 

diskdef z9001
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 192
  skew 0
  boottrk 0
  os 2.2
end 

# Visual Technology Visual 1050 computer
diskdef v1050
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 3
end

# Microbee 40 track 5.25" disks
diskdef microbee40
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 128
  skewtab 1,4,7,0,3,6,9,2,5,8
  boottrk 2
  os 2.2
end

diskdef dreamdisk40
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 128
  skewtab 1,4,7,0,3,6,9,2,5,8
  boottrk 2
  os 2.2
end

diskdef dreamdisk80
  seclen 512
  tracks 160
  sectrk 10
  blocksize 2048
  maxdir 256
  skewtab 1,4,7,0,3,6,9,2,5,8
  boottrk 2
  os 2.2
end

# RC75x series
diskdef rc75x
  seclen 1024
  tracks 154
  sectrk 8
  blocksize 2048
  maxdir 512
  boottrk 4
  os 3
end

# ICL Comet: 40 track 5.25" Single Sided
#
diskdef icl-comet-525ss
   seclen 512
   tracks 40
   sectrk 10
   blocksize 1024
   maxdir 64
   skewtab 0,3,6,9,2,5,8,1,4,7
   boottrk 2
   os 2.2
end

diskdef z80pack-hd
  seclen 128
  tracks 255
  sectrk 128
  blocksize 2048
  maxdir 1024
  skew 0
  boottrk 0
  os 2.2
end

diskdef z80pack-hdb
  seclen 128
  tracks 256
  sectrk 16384
  blocksize 16384
  maxdir 8192
  skew 0
  boottrk 0
  os 2.2
end

# Bondwell 12 and 14 disk images in IMD raw binary format
diskdef bw12
  seclen 256
  tracks 40
  sectrk 18
  blocksize 2048
  maxdir 64
  skew 1
  boottrk 2
  os 2.2
end

diskdef bw14
  seclen 256
  tracks 80
  sectrk 18
  blocksize 2048
  maxdir 64
  skew 1
  boottrk 2
  os 2.2
end

############################
# north star cp/m  disks
############################

#North Star floppy 360K

diskdef nsfd
  seclen 512
  tracks 70 
  sectrk 10 
  blocksize 2048
  maxdir 64
  skew 5  
  boottrk 2
  os 2.2
end


#North Star CP/M Virtual-Disk file on Hard Disk
# prepared with allocation factor = 4
# as in "CR CPMB 4000 4"
# needs to be copied off hard drive before you can 
# work on it with cpmtools

diskdef nshd4
  seclen 512
  tracks 512
  sectrk 16 
  blocksize 4096
  maxdir 256
  skew 0  
  boottrk 0
  os 2.2
end


#North Star CP/M Virtual-Disk file on Hard Disk
# prepared with allocation factor = 8
# as in "CR CPMB 6000 8"
# needs to be copied off hard drive before you can
# work on it with cpmtools

diskdef nshd8
  seclen 512
  tracks 1024
  sectrk 16 
  blocksize 8192
  maxdir 256
  skew 0  
  boottrk 0
  os 2.2
end

# Northstar Micro-Disk System MDS-A-D 175
diskdef mdsad175
    seclen 512
    blocksize 1024
    tracks 35
    maxdir 64
    boottrk 2
    sectrk 10
    skew 5
    os 2.2
end


# Northstar Micro-Disk System MDS-A-D 350
diskdef mdsad350
   seclen 512
   blocksize 2048
   tracks 70
   maxdir 64
   boottrk 2
   sectrk 10
   skew 5
   os 2.2
end


# Osborne 1
diskdef osborne1
   seclen 1024
   tracks 40
   sectrk 5
   blocksize 1024
   maxdir 64
   boottrk 3
   os 2.2
end

# Osborne Nuevo/Vixen/4
diskdef osborne4
   seclen 1024
   tracks 80
   sectrk 5
   blocksize 2048
   maxdir 128
   skew 2
   boottrk 2
   os 2.2
end

# Lobo Max-80 8" CP/M 2
diskdef lobo2
  seclen 256
  tracks 77
  sectrk 30
  blocksize 2048
  maxdir 64
  skew 0
  boottrk 2
  os 2.2
end

#Lobo Max-80 8" CP/M 3
diskdef lobo3
  seclen 512
  tracks 77
  sectrk 17
  blocksize 2048
  maxdir 64
  skew 0
  boottrk 2
  os 3
end

# PRO CP/M RZ50 DZ format (Perhaps only 79 tracks should be used?)
diskdef dec_pro
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 128
  skew 2
  boottrk 2
  os 2.2
end

# TDOS with DateStamper
diskdef tdos-ds
  seclen 1024
  tracks 77
  sectrk 16
  blocksize 2048
  maxdir 256
  skew 0
  boottrk 1
  os zsys
end

# The following entires are tested and working
# Most of the images are either from Don Maslin's archive or from
# Dave Dunfield's site, but not all - they are noted as well as
# their size.

# PMC Micromate
# Dave Dunfield's Imagedisk information from DSK conversion from IMD:
# IMageDisk Utility 1.18 / Mar 07 2012
# IMD 1.14: 10/03/2007 11:13:27
# PMC-101 MicroMate
# CP/M Plus
# System Master
# Assuming 1:1 for Binary output
# 0/0 250 kbps DD  5x1024
# 80 tracks(40/40), 400 sectors (12 Compressed)
# Entry derived from above - image size = 409,600, from Dave Dunfield
diskdef pmc101
  seclen 1024
  tracks 80
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 3
end
  
# BEGIN td143ssdd8  Turbo Dos 1.43 - SSDD 8" - 512 x 16
# Test OK - image size = 630,784, from Don Maslin's archive
diskdef td143ssdd8
  seclen 512
  tracks 77
  sectrk 9
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 0
  os 2.2
# DENSITY MFM ,LOW 
end

# BEGIN headsdd8  Heath H89, Magnolia CP/M - SSDD 8" - 512 x 16
# Test OK - image size = 630,784, from Don Maslin's archive
diskdef heassdd8
  seclen 512
  tracks 77
  sectrk 16
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
# DENSITY MFM ,LOW 
end

# ZEN7  Zenith Z-100 - SSDD 48 tpi 5.25" - 512 x 8
diskdef zen7
  seclen 512
  tracks 40
  sectrk 8
  blocksize 1024
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# ZEN8  Zenith Z-100 - DSDD 48 tpi 5.25" - 512 x 8
diskdef zen8
  seclen 512
  tracks 80
  sectrk 8
  blocksize 2048
  maxdir 256
  skew 1
  boottrk 2
  os 2.2
end

# ZEN9  Zenith Z-100 - SSSD 8" - 128 x 26
diskdef zen9
  seclen 128
  tracks 77
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 6
  boottrk 2
  os 2.2
end

# ZENA  Zenith Z-100 - SSDD 8" - 256 x 26
diskdef zena
  seclen 256
  tracks 77
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 9
  boottrk 2
  os 2.2
end

# Morrow Designs Micro-Decision         DOUBLE
# 64k CP/M Vers. 2.2 Rev.2.3            SIDED
# Copyright '76, '77, '78, '79, '80
# Digital Research
# Copyright 1982,1983 Morrow Designs, Inc.
# Assuming 1:1 for Binary output
#  0/0 250 kbps DD  5x1024
# 80 tracks(40/40), 400 sectors (128 Compressed)
# Entry derived from above data
# Test OK - image siae = 409600, from Dave Dunfield
diskdef mordsdd
  seclen 1024
  tracks 80
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 3
  boottrk 2
  OS 2.2
end


# BEGIN morsddd Morrow MD2 - SSDD 48 tpi 5.25" - 1024 x 5
# Test OK - image size = 204,800, from Don Maslin's archive
# Also tested with image from Dave Dunfield
diskdef morsddd
  seclen 1024
  tracks 40
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 3
  boottrk 2
  os 2.2
# DENSITY MFM ,LOW 
# BSH 4 BLM 15 EXM 1 DSM 94 DRM 127 AL0 0C0H AL1 0 OFS 2
end

# BEGIN osb1sssd  Osborne 1 - SSSD 48 tpi 5.25" - 256 x 10
# Test OK - image size = 102,400, from Don Maslin's archive
diskdef osb1sssd
  seclen 256
  tracks 40
  sectrk 10
  blocksize 2048
  maxdir 64
  skew 2
  boottrk 3
  os 2.2
# DENSITY MFM ,LOW 
# BSH 4 BLM 15 EXM 1 DSM 45 DRM 63 AL0 080H AL1 0 OFS 3
end

# BEGIN altdsdd  Altos - DSDD 5" - 512 x 9
# Test OK - both CP/M and MP/M - image size = 737,280, from Dave Dunfield
diskdef altdsdd
  seclen 512
  tracks 160
  sectrk 9
  blocksize 4096
  maxdir 177
  skew 0
  boottrk 2
  os 3
# DENSITY MFM ,HIGH 
# BSH 5 BLM 31 EXM 3 DSM 176 DRM 176 AL0 0C0H AL1 0 OFS 2
end

# All TRS formats added by Larry Kraemer

# BEGIN trsomsssd  TRS-80 Model 1, Omikron CP/M - SSSD 48 tpi 5.25" - 128 x 18
# Test OK - image size = 80,640, from TRS-80 Yahoo Group posting
diskdef trsomsssd
  seclen 128
  tracks 35
  sectrk 18
  blocksize 1024
  maxdir 64
  skew 4
  boottrk 3
  os 2.2
# DENSITY FM ,LOW 
# BSH 3 BLM 7 EXM 0 DSM 71 DRM 63 AL0 0C0H AL1 0 OFS 3
end

diskdef trsg         #= TRS-80 Model 4,4P Montezuma System 170K - SSDD 48 tpi 5.25"
  seclen 256         #= Sectors xx,256
  tracks 40          #= (Cylinders * Sides) = 40*1 = 40
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 18          #= Sectors 18,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsh         #= TRS-80 Model 4,4P Montezuma Data 200K - SSDD 48 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 40          #= (Cylinders * Sides) = 40*1 = 40
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsi         #= TRS-80 Model 4,4P Montezuma System 350K - DSDD 48 tpi 5.25"
  seclen 256         #= Sectors xx,256
  tracks 80          #= (Cylinders * Sides) = 40*2 = 80
#  sides outout       #= Order of Cylinders  = alt, outout, outback
  sectrk 18          #= Sectors 18,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
#end

diskdef trsj         #= TRS-80 Model 4,4P Montezuma Data 400K - DSDD 48 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 80          #= (Cylinders * Sides) = 40*2 = 80
#  sides outout       #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsk         #= TRS-80 Model 4,4P Montezuma System 350K - SSDD 96 tpi 5.25"
  seclen 256         #= Sectors xx,256
  tracks 80          #= (Cylinders * Sides) = 80*1 = 80
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 18          #= Sectors 18,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsl         #= TRS-80 Model 4,4P Montezuma Data 400K - SSDD 96 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 80          #= (Cylinders * Sides) = 80*1 = 80
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsm         #= TRS-80 Model 4,4P Montezuma System 710K - DSDD 96 tpi 5.25"
  seclen 256         #= Sectors xx,256
  tracks 160         #= (Cylinders * Sides) = 80*2 = 160
#  sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 18          #= Sectors 18,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsn         #= TRS-80 Model 4,4P Montezuma Data 800K - DSDD 96 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 160         #= (Cylinders * Sides) = 80*2 = 160
#  sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 0             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trso         #= TRS-80 Model 4,4P Montezuma Extend System 190K - SSDD 48 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 40          #= (Cylinders * Sides) = 40*1 = 40
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try x
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsp         #= TRS-80 Model 4,4P Montezuma Extend System 390K - DSDD 48 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 80          #= (Cylinders * Sides) = 40*2 = 80
#  sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsq         #= TRS-80 Model 4,4P Montezuma Extend System 390K - SSDD 96 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 80          #= (Cylinders * Sides) = 80*1 = 80
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsr         #= TRS-80 Model 4,4P Montezuma Extend System 790K - DSDD 96 tpi 5.25"
  seclen 512         #= Sectors xx,512
  tracks 160         #= (Cylinders * Sides) = 80*2 = 160
#  sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 2          #= OFS = 2
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trss         #= TRS-80 Model 4,4P Montezuma Super Data 220K - SSDD 48 tpi 5.25"
  seclen 1024        #= Sectors xx,1024
  tracks 40          #= (Cylinders * Sides) = 40*1 = 40
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 6           #= Sectors 6,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trst         #= TRS-80 Model 4,4P Montezuma Super Data 440K - DSDD 48 tpi 5.25"
  seclen 1024        #= Sectors xx,1024
  tracks 80          #= (Cylinders * Sides) = 40*2 = 80
#  sides outout       #= Order of Cylinders  = alt, outout, outback
  sectrk 6           #= Sectors 6,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsu         #= TRS-80 Model 4,4P Montezuma Super Data 440K - SSDD 96 tpi 5.25"
  seclen 1024        #= Sectors xx,1024
  tracks 80          #= (Cylinders * Sides) = 80*1 = 80
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 6           #= Sectors 6,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsv         #= TRS-80 Model 4,4P Montezuma Super Data 880K - DSDD 96 tpi 5.25"
  seclen 1024        #= Sectors xx,1024
  tracks 160         #= (Cylinders * Sides) = 80*2 = 160
#  sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 6           #= Sectors 6,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try x
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

diskdef trsw         #= TRS-80 Model 4,4P Montezuma System 400K - SSDD 96 tpi 3.5"
  seclen 512         #= Sectors xx,512
  tracks 80          #= (Cylinders * Sides) = 80*1 = 80
# sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 10          #= Sectors 10,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
#  datarate DD        #= DENSITY SD, DD, HD, or ED
#  FM NO              #= Format YES = FM, or NO = MFM
  skew 2             #= [0..8] try 2
  boottrk 0          #= OFS = 0
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

#BEGIN TRSE  TRS-80 II/12/16 Aton CP/M - SSHD 8" - 1024 x 8
diskdef trse
  seclen 1024
  tracks 77
  sectrk 8
  blocksize 2048
  maxdir 128
  datarate DD
  fm NO
  skew 3
  boottrk 0
  offset 11520
  os 2.2
end

# TRSF  TRS-80 II/12/16 Aton CP/M  - DSHD 8" - 1024 x 8
diskdef trsf
  seclen 1024
  tracks 154
  sides alt
  sectrk 8
  blocksize 2048
  maxdir 192
  skew 3
  boottrk 0
  offset 11520
  os 2.2
end

# TRS5  TRS-80, Lifeboat CP/M (1024 bytes/sector) - SSDD 8"
# The first track is 26 sectors with 128 bytes, the rest are 1024 x 8
diskdef trs5
  seclen 1024
  tracks 75
  sectrk 8
  blocksize 2048
  maxdir 128
  skew 3
  boottrk 0
  os 2.2
  offset 11520
end

# Memotech type 03, ie: 3.5" or 5.25", D/S, D/D, S/T
# 40 tracks, 2 sides, 16 sectors/track, 256 bytes/sector
# Bytes on the media = 2*40*16*256 = 327680
# CP/M sees 26 128 byte records per track (similar to 8" disks).
# Tracks = 327680/(26*128) = 98
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = ((98-2)*26*128)/2048 = 156, which agrees with DPB

diskdef memotech-type03
  seclen 128
  tracks 98
  sectrk 26
  blocksize 2048
  maxdir 64
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 07, ie: 3.5" or 5.25", D/S, D/D, D/T
# 80 tracks, 2 sides, 16 sectors/track, 256 bytes/sector
# Bytes on the media = 2*80*16*256 = 655360
# CP/M sees 26 128 byte records per track (similar to 8" disks).
# Tracks = 655360/(26*128) = 196
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = ((196-2)*26*128)/2048 = 315, which agrees with DPB

diskdef memotech-type07
  seclen 128
  tracks 196
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 43, ie: 1MB Silicon Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for Silicon Discs includes blocks on the last incomplete track
# Tracks = 1048576/(26*128) = 315.07
# Data is in 4096 byte blocks, on track 2 onwards
# Blocks = (1048576-2*26*128)/4096 = 254, which agrees with DPB
# Blocks = ((315-2)*26*128)/4096 = 254, so we don't need the 0.07 track
diskdef memotech-type43
  seclen 128
  tracks 315
  sectrk 26
  blocksize 4096
  maxdir 256
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 47, ie: 2MB Silicon Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for Silicon Discs includes blocks on the last incomplete track
# Tracks = 2097152/(26*128) = 630.15
# Data is in 4096 byte blocks, on track 2 onwards
# Blocks = (2097152-2*26*128)/4096 = 510, which agrees with DPB
# Blocks = ((630-2)*26*128)/4096 = 510, so we don't need the 0.15 track
diskdef memotech-type47
  seclen 128
  tracks 630
  sectrk 26
  blocksize 4096
  maxdir 256
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 4B, ie: 4MB Silicon Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for Silicon Discs includes blocks on the last incomplete track
# Tracks = 4194304/(26*128) = 1260.3
# Data is in 4096 byte blocks, on track 2 onwards
# Blocks = (4194304-2*26*128)/4096 = 1022, which agrees with DPB
# Blocks = ((1260-2)*26*128)/4096 = 1022, so we don't need the 0.3 track
diskdef memotech-type4B
  seclen 128
  tracks 1260
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 4F, ie: 8MB Silicon Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for Silicon Discs includes blocks on the last incomplete track
# Tracks = 8388608/(26*128) = 2520.61
# Data is in 4096 byte blocks, on track 2 onwards
# Blocks = (8388608-2*26*128)/4096 = 2046, which agrees with DPB
# Blocks = ((2520-2)*26*128)/4096 = 2045, so we need the extra 0.61 track
diskdef memotech-type4F
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 18, ie: 8MB SD Card
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for SD Cards includes blocks on the last incomplete track
# Tracks = 8388608/(26*128) = 2520.61
# Data is in 4096 byte blocks, on track 2 onwards
# Blocks = (8388608-2*26*128)/4096 = 2046, which agrees with DPB
# Blocks = ((2520-2)*26*128)/4096 = 2045, so we need the extra 0.61 track
diskdef memotech-type18
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 19, ie: 8MB SD Card
diskdef memotech-type19
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 8M
end

# Memotech type 1A, ie: 8MB SD Card
diskdef memotech-type1A
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 16M
end

# Memotech type 1B, ie: 8MB SD Card
diskdef memotech-type1B
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 24M
end

# Memotech type 1C, ie: 8MB SD Card
diskdef memotech-type1C
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 32M
end

# Memotech type 1D, ie: 8MB SD Card
diskdef memotech-type1D
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 40M
end

# Memotech type 1E, ie: 8MB SD Card
diskdef memotech-type1E
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 48M
end

# Memotech type 1F, ie: 8MB SD Card
diskdef memotech-type1F
  seclen 128
  tracks 2521
  sectrk 26
  blocksize 4096
  maxdir 512
  skew 1
  boottrk 2
  os 2.2
  offset 56M
end

# Memotech type 50, ie: 256KB RAM Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for RAM Discs includes blocks on the last incomplete track
# Tracks = 262144/(26*128) = 78.76
# Data is in 1024 byte blocks, on track 2 onwards
# Blocks = (262144-2*26*128)/1024 = 249, which agrees with DPB 
# Blocks = ((78-2)*26*128)/1024 = 247, so we need the extra 0.76 track
diskdef memotech-type50
  seclen 128
  tracks 79
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 51, ie: 512KB RAM Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for RAM Discs includes blocks on the last incomplete track
# Tracks = 524288/(26*128) = 157.53
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = (524288-2*26*128)/2048 = 252, which agrees with DPB
# Blocks = ((157-2)*26*128)/2048 = 251, so we need the extra 0.53 track
diskdef memotech-type51
  seclen 128
  tracks 158
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 51, as used in Italy, ie: 480KB RAM Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for RAM Discs includes blocks on the last incomplete track
# Tracks = 491520/(26*128) = 147.69
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = (491520-2*26*128)/2048 = 236, which agrees with DPB
# Blocks = ((147-2)*26*128)/2048 = 235, so we need the extra 0.69 track
diskdef memotech-type51-italy
  seclen 128
  tracks 148
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 51, after S2R64.COM, ie: 448KB RAM Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for RAM Discs includes blocks on the last incomplete track
# Tracks = 458752/(26*128) = 137.84
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = (458752-2*26*128)/2048 = 220, which agrees with DPB, after S2R64.COM
# Blocks = ((137-2)*26*128)/2048 = 219, so we need the extra 0.84 track
diskdef memotech-type51-s2r64
  seclen 128
  tracks 138
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 51, after S2R.COM, ie: 144KB RAM Disc
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for RAM Discs includes blocks on the last incomplete track
# Tracks = 147456/(26*128) = 44.3
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = (147456-2*26*128)/2048 = 68, which agrees with DPB, after S2R.COM
# Blocks = ((44-2)*26*128)/2048 = 68, so we don't need the extra 0.3 track
diskdef memotech-type51-s2r
  seclen 128
  tracks 44
  sectrk 26
  blocksize 2048
  maxdir 128
  skew 1
  boottrk 2
  os 2.2
end

# Memotech type 52, ie: 320KB RAM Disc
# Added for REMEMOTECH
# CP/M sees 26 128 byte records per track
# Note: Unlike common practice with real physical disks, with real geometry,
#       the DPB for RAM Discs includes blocks on the last incomplete track
# Tracks = 327680/(26*128) = 98.46
# Data is in 2048 byte blocks, on track 2 onwards
# Blocks = (327680-2*26*128)/2048 = 156
# Blocks = ((98-2)*26*128)/2048 = 156, so we don't need the extra 0.46 track
# This type very deliberately and conveniently exactly matches type 03
diskdef memotech-type52
  seclen 128
  tracks 98
  sectrk 26
  blocksize 2048
  maxdir 64
  skew 1
  boottrk 2
  os 2.2
end

# Research Machines 380Z/480Z 5.25" "Single Density" or "MDS" format.
# All tracks are formatted FM 16x128.
diskdef rm-sd
  seclen 128
  tracks 40
  sectrk 16
  blocksize 1024
  maxdir 64
  skew 3
  boottrk 3
  os 2.2
end

# Research Machines 380Z/480Z 5.25" "Double Density" or "MD" format.
# Track 0 is formatted FM 16x128; 1+ are MFM 9x512.
# If you're working with an image file, make sure that track 0 is
# padded to be the same size as the other tracks.
diskdef rm-dd
  seclen 512
  tracks 40
  sectrk 9
  blocksize 1024
  maxdir 64
  skew 5
  boottrk 3
  os 2.2
end

# Research Machines 380Z/480Z 5.25" "Quad Density" or "MQ" format.
# Track 0 is formatted FM 16x128; 1+ are MFM 9x512.
diskdef rm-qd
  seclen 512
  tracks 80
  sectrk 9
  blocksize 2048
  maxdir 128
  skew 5
  boottrk 3
  os 2.2
end

# Ampro Little Board Z80 running CP/M 2.21
# BEGIN AMP1  Ampro - SSDD 48 tpi 5.25"
# DENSITY MFM, LOW
# CYLINDERS 40 SIDES 1 SECTORS 10,512 SKEW 2
# SIDE1 0 1,2,3,4,5,6,7,8,9,10
# BSH 4 BLM 15 EXM 1 DSM 94 DRM 63 AL0 080H AL1 0 OFS 2
# END

diskdef amp1
  seclen 512       #= Sectors xx,512
  tracks 40         #= (Cylinders * Sides) = 40*1 = 40
  sectrk 10         #= Sectors 10,xxx
  blocksize 2048 #= (128*(BLM+1)) = 2048
  maxdir 64         #(DRM+1) = 64
  skew 0             #= SKEW = 0
  boottrk 2           #= OFS = 2
  os 2.2
end

#BEGIN AMP2  Ampro - DSDD 48 tpi 5.25"
#DENSITY MFM, LOW
#CYLINDERS 40 SIDES 2
#SECTORS 10,512
#SKEW 2
#SIDE1 0 17,18,19,20,21,22,23,24,25,26
#SIDE2 1 17,18,19,20,21,22,23,24,25,26
#ORDER SIDES
#BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
#END

# setfdprm /dev/fd0 DS DD ssize=512 cyl=40 sect=10 head=2
diskdef amp2
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

#BEGIN AMP3  Ampro - SSDD 96 tpi 3.5"
#DENSITY MFM, LOW
#CYLINDERS 80 SIDES 1 SECTORS 5,1024 SKEW 2
#SIDE1 0 1,2,3,4,5
#BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
#END

# setfdprm /dev/fd0 SS DD ssize=1024 cyl=80 sect=5 head=1
diskdef amp3
  seclen 1024
  tracks 80
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

#BEGIN AMP4  Ampro - DSDD 96 tpi 3.5"
#DENSITY MFM, LOW
#CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
#SIDE1 0 17,18,19,20,21
#SIDE2 1 17,18,19,20,21
#ORDER SIDES
#BSH 4 BLM 15 EXM 0 DSM 394 DRM 255 AL0 0F0H AL1 0 OFS 2
#END

# setfdprm /dev/fd0 DS DD ssize=1024 cyl=80 sect=5 head=2
diskdef amp4
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 256
  skew 0
  boottrk 2
  os 2.2
end

#BEGIN AMP5  Ampro - SSDD 3.5"
#DENSITY MFM, LOW
#CYLINDERS 80 SIDES 1 SECTORS 5,1024 SKEW 2
#SIDE1 0 1,2,3,4,5
#BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
#END

# setfdprm /dev/fd0 SS DD ssize=1024 cyl=80 sect=5 head=1
diskdef amp5
  seclen 1024
  tracks 80
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

#BEGIN AMP6  Ampro - DSDD 3.5"
#DENSITY MFM, LOW
#CYLINDERS 80 SIDES 2 SECTORS 5,1024 SKEW 2
#SIDE1 0 17,18,19,20,21
#SIDE2 1 17,18,19,20,21
#ORDER SIDES
#BSH 4 BLM 15 EXM 0 DSM 394 DRM 255 AL0 0F0H AL1 0 OFS 2
#END

# setfdprm /dev/fd0 DS DD ssize=1024 cyl=80 sect=5 head=2
diskdef amp6
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 256
  skew 0
  boottrk 2
  os 2.2
end

diskdef ampro800
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 256
  skew 0
  boottrk 2
  os 2.2
end

# Ampro - DSDD 48 tpi 5.25" - 512 x 10
diskdef ampro400d
  seclen 512
  tracks 80
  sectrk 10
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
  libdsk:format ampro400d
# DENSITY MFM ,LOW 
# BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
end

# BEGIN ampdsdd80  Ampro - DSDD 96 tpi 5.25" - 512 x 10
# Test OK - image size = 819,200, from Don Maslin's archive
diskdef ampdsdd80
  seclen 1024
  tracks 160
  sectrk 5
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
  libdsk:format ampro800
# DENSITY MFM ,LOW 
# BSH 4 BLM 15 EXM 1 DSM 194 DRM 127 AL0 0C0H AL1 0 OFS 2
end

# ALTAIRZ80 SIMH *dsk 8MB Harddisk (Type AZ80 HDSK)
diskdef 8megAltairSIMH
  seclen 128
  tracks 2048
  sectrk 32
  blocksize 4096
  maxdir 1024
  skew 0
  boottrk 6
  os 2.2
end

# ALTAIRZ80 SIMH *dsk MITS 88-DISK 137 Byte/Sektor
# speedball (copylib) skewtable
diskdef simh
  seclen 128
  tracks 254
  sectrk 32
  blocksize 2048
  maxdir 256
  skew 17
  boottrk 6
  os 2.2
end

diskdef all1         #= Allen-Bradley Advisor+ - DSDD 3.5"
  seclen 512         #= Sectors xx,512
  tracks 160         #= (Cylinders * Sides) = 80*2 = 160
  sides alt          #= Order of Cylinders  = alt, outout, outback
  sectrk 8           #= Sectors 8,xxx
  blocksize 2048     #= (128*(BLM+1)) =  7=1024, 15=2048, 31=4096, 63=8192
  maxdir 128         #= (DRM+1) = 128
  datarate DD        #= DENSITY SD, DD, HD, or ED
  FM NO              #= Format YES = FM, or NO = MFM
  skew 0             #= [0..8] try x
  boottrk 1          #= OFS = 1
#                    #= 2, 2.2, or 3 (NO comment on next line)
  os 2.2
end

# COM8  Compupro (Viasyn) 8/16 - SSDD 8" - 1024 x 8
# IMD RAW format
diskdef com8
  seclen 1024
  tracks 77
  sectrk 8
  blocksize 2048
  maxdir 128
  skew 3
  offset 11520
  boottrk 0
  os 2.2
end

# Spectravideo SVI-728 (MSX) with SVI-707 floppy drive
diskdef svi707
  seclen 256
  tracks 40
  sectrk 17
  blocksize 2048
  maxdir 64
  skew 0
  boottrk 3
  os 2.2
end

# Intel MDS/22 8" Double Density
diskdef mds-dd
  seclen 128
  tracks 77
  sectrk 52
  blocksize 2048
  maxdir 128
  skew 0
  boottrk 2
  os 2.2
end

# Intel MDS/22 8" Single Density. Untested.
diskdef mds-sd
  seclen 128
  tracks 77
  sectrk 26
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 2
  os 2.2
end

# CF card in PCMCIA slot on NC200 with cpmish
diskdef nc200cf
  seclen 512
  tracks 256
  sectrk 256
  blocksize 16384
  maxdir 512
  boottrk 0
  os 2.2
end

# Floppy image on NC200 with cpmish
diskdef nc200cpm
  seclen 512
  tracks 80
  sectrk 18
  blocksize 2048
  maxdir 128
  boottrk 2
  os 2.2
end

# ZCN format drive partitions in nc100em's nc100.card
# use this for a bootable A: drive
# (assumes ZCN system is 12k, which it has been for years)
diskdef zcna_boot
  seclen 1024
  tracks 256
  sectrk 1
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 13
  os 2.2
end

# use this for a non-bootable A: drive
diskdef zcna_nonboot
  seclen 1024
  tracks 256
  sectrk 1
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 1
  os 2.2
end

# ZCN b/c/d all assumed to be non-bootable
diskdef zcnb
  seclen 1024
  tracks 256
  sectrk 1
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 1
  os 2.2
  offset 256KB
end

diskdef zcnc
  seclen 1024
  tracks 256
  sectrk 1
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 1
  os 2.2
  offset 512KB
end

diskdef zcnd
  seclen 1024
  tracks 256
  sectrk 1
  blocksize 1024
  maxdir 64
  skew 0
  boottrk 1
  os 2.2
  offset 768KB
end

# Hewlett-Packard HP9000-200 - 70-track SS drive that emulates a
# 35 track DSDD 48 tpi 5.25"
diskdef HP25
  seclen 256
  tracks 66
  sectrk 16
  blocksize 1024
  maxdir 128
  skew 0
  boottrk 3
  os 2.2
end



diskdef yaze512
# BSH 4 BLM 15 EXM 1 DSM 255 DRM 1023 AL0 0FFH AL1 0FFH OFS 0
seclen 128
tracks 4096
sectrk 8
blocksize 2048
maxdir 1024
skew 1
offset 128
boottrk 0
os 3
end
